//===- SparcV9_F3.td - SparcV9 Format 3 Instructions -------*- tablegen -*-===//
// 
//                     The LLVM Compiler Infrastructure
//
// This file was developed by the LLVM research group and is distributed under
// the University of Illinois Open Source License. See LICENSE.TXT for details.
// 
//===----------------------------------------------------------------------===//

//===----------------------------------------------------------------------===//
// Format #3 classes
//

// F3 - Common superclass of all F3 instructions.  All instructions have an op3
// field.
class F3 : InstV9 {
  bits<6> op3;
  let op{1} = 1;   // Op = 2 or 3
  let Inst{24-19} = op3;
}

// F3_rs1 - Common class of instructions that have an rs1 field
class F3_rs1 : F3 {
  bits<5> rs1;
  let Inst{18-14} = rs1;
}

// F3_rs1rs2 - Common class of instructions that only have rs1 and rs2 fields
class F3_rs1rs2 : F3_rs1 {
  bits<5> rs2;
  let Inst{4-0} = rs2;
}

// F3_rs1rs2 - Common class of instructions that only have rs1 and rs2 fields
class F3_rs1rs2rd : F3_rs1rs2 {
  bits<5> rd;
  let Inst{29-25} = rd;
}

// F3_rs1simm13 - Common class of instructions that only have rs1 and simm13
class F3_rs1simm13 : F3_rs1 {
  bits<13> simm13;
  let Inst{12-0} = simm13;
}

class F3_rs1simm13rd : F3_rs1simm13 {
  bits<5> rd;
  let Inst{29-25} = rd;
}

// F3_rs1rd - Common class of instructions that have an rs1 and rd fields
class F3_rs1rd : F3_rs1 {
  bits<5> rd;
  let Inst{29-25} = rd;
}

// F3_rs2 - Common class of instructions that don't use an rs1
class F3_rs2 : F3 {
  bits<5> rs2;
  let Inst{4-0} = rs2;
}

// F3_rs2rd - Common class of instructions that use rs2 and rd, but not rs1
class F3_rs2rd : F3_rs2 {
  bits<5> rd;
  let Inst{29-25} = rd;
}

// F3_rd - Common class of instructions that have an rd field
class F3_rd : F3 {
  bits<5> rd;
  let Inst{29-25} = rd;
}

// F3_rdrs1 - Common class of instructions that have rd and rs1 fields
class F3_rdrs1 : F3_rd {
  bits<5> rs1;
  let Inst{18-14} = rs1;
}

// F3_rdrs1simm13 - Common class of instructions that have rd, rs1, and simm13
class F3_rdrs1simm13 : F3_rdrs1 {
  bits<13> simm13;
  let Inst{12-0} = simm13;
}

// F3_rdrs1rs2 - Common class of instructions that have rd, rs1, and rs2 fields
class F3_rdrs1rs2 : F3_rdrs1 {
  bits<5> rs2;
  let Inst{4-0} = rs2;
}


// Specific F3 classes...
//

class F3_1<bits<2> opVal, bits<6> op3val, string name> : F3_rs1rs2rd {
  let op  = opVal;
  let op3 = op3val;
  let Name = name;
  let Inst{13} = 0;   // i field = 0
  let Inst{12-5} = 0; // don't care
}

// The store instructions seem to like to see rd first, then rs1 and rs2
class F3_1rd<bits<2> opVal, bits<6> op3val, string name> : F3_rdrs1rs2 {
  let op  = opVal;
  let op3 = op3val;
  let Name = name;
  let Inst{13} = 0;   // i field = 0
  let Inst{12-5} = 0; // don't care
}

class F3_2<bits<2> opVal, bits<6> op3val, string name> : F3_rs1simm13rd {
  let op  = opVal;
  let op3 = op3val;
  let Name = name;
  let Inst{13} = 1;   // i field = 1
}

// The store instructions seem to like to see rd first, then rs1 and imm
class F3_2rd<bits<2> opVal, bits<6> op3val, string name> : F3_rdrs1simm13 {
  let op  = opVal;
  let op3 = op3val;
  let Name = name;
  let Inst{13} = 1;   // i field = 1
}

class F3_3<bits<2> opVal, bits<6> op3val, string name> : F3_rs1rs2 {
  let op   = opVal;
  let op3  = op3val;
  let Name = name;
  let Inst{29-25} = 0; // don't care
  let Inst{13} = 0;    // i field = 0
  let Inst{12-5} = 0;  // don't care
}

class F3_4<bits<2> opVal, bits<6> op3Val, string name> : F3_rs1simm13 {
  let op   = opVal;
  let op3  = op3Val;
  let Name = name;
  let Inst{29-25} = 0; // don't care
  let Inst{13} = 1;    // i field = 1
  let Inst{12-0} = simm13;
}

class F3_5<bits<2> opVal, bits<6> op3Val, bits<3> rcondVal,
           string name> : F3_rs1rs2rd {
  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{13} = 0;           // i field = 0
  let Inst{12-10} = rcondVal; // rcond field
  let Inst{9-5} = 0;          // don't care
}

class F3_6<bits<2> opVal, bits<6> op3Val, bits<3> rcondVal,
           string name> : F3_rs1 {
  bits<10> simm10;
  bits<5>  rd;

  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{29-25} = rd;
  let Inst{13} = 1;           // i field = 1
  let Inst{12-10} = rcondVal; // rcond field
  let Inst{9-0} = simm10;
}

//FIXME: classes 7-10 not defined!!

class F3_11<bits<2> opVal, bits<6> op3Val, string name> : F3_rs1rs2rd {
  bit x;
  let op = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{13} = 0; // i field = 0
  let Inst{12} = x;
  let Inst{11-5} = 0; // don't care
}

class F3_12<bits<2> opVal, bits<6> op3Val, string name> : F3_rs1 {
  bits<5> shcnt;
  bits<5> rd;

  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{29-25} = rd;
  let Inst{13} = 1; // i field = 1
  let Inst{12} = 0; // x field = 0
  let Inst{11-5} = 0; // don't care
  let Inst{4-0} = shcnt;
}

class F3_13<bits<2> opVal, bits<6> op3Val, string name> : F3_rs1 {
  bits<6> shcnt;
  bits<5> rd;

  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{29-25} = rd;
  let Inst{13} = 1; // i field = 1
  let Inst{12} = 1; // x field = 1
  let Inst{11-6} = 0; // don't care
  let Inst{5-0} = shcnt;
}

class F3_14<bits<2> opVal, bits<6> op3Val,
            bits<9> opfVal, string name> : F3_rs2rd {
  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{18-14} = 0; // don't care
  let Inst{13-5} = opfVal;
}

class F3_15<bits<2> opVal, bits<6> op3Val,
            bits<9> opfVal, string name> : F3 {
  bits<2> cc;
  bits<5> rs1;
  bits<5> rs2;

  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{29-27} = 0; // defined to be zero
  let Inst{26-25} = cc;
  let Inst{18-14} = rs1;
  let Inst{13-5}  = opfVal;
  let Inst{4-0}   = rs2;
}
  
class F3_16<bits<2> opVal,  bits<6> op3Val,
            bits<9> opfval, string name> : F3_rs1rs2rd {
  let op  = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{13-5} = opfval;
}

class F3_17<bits<2> opVal, bits<6> op3Val, string name> : F3_rs1rd {
  let op = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{13-0} = 0; // don't care
}

class F3_18<bits<5> fcn, string name> : F3 {
  let op = 2;
  let op3 = 0b111110;
  let Name = name;
  let Inst{29-25} = fcn;
  let Inst{18-0 } = 0; // don't care;
}

class F3_19<bits<2> opVal, bits<6> op3Val, string name> : F3_rd {
  let op = opVal;
  let op3 = op3Val;
  let Name = name;
  let Inst{18-0} = 0; // don't care
}

// FIXME: class F3_20
// FIXME: class F3_21
