"LAMMPS WWW Site"_lws - "LAMMPS Documentation"_ld - "LAMMPS Commands"_lc :c

:link(lws,http://lammps.sandia.gov)
:link(ld,Manual.html)
:link(lc,Section_commands.html#comm)

:line

compute smd/tlsph/dt command :h3

[Syntax:]

compute ID group-ID smd/tlsph/dt :pre

ID, group-ID are documented in "compute"_compute.html command
smd/tlsph/dt = style name of this compute command :ul

[Examples:]

compute 1 all smd/tlsph/dt :pre

[Description:]

Define a computation that outputs the CFL-stable time increment per
particle.  This time increment is essentially given by the speed of
sound, divided by the SPH smoothing length.  Because both the speed of
sound and the smoothing length typically change during the course of a
simulation, the stable time increment needs to be recomputed every
time step.  This calculation is performed automatically in the
relevant SPH pair styles and this compute only serves to make the
stable time increment accessible for output purposes.

See "this PDF guide"_PDF/SMD_LAMMPS_userguide.pdf to using Smooth
Mach Dynamics in LAMMPS.

[Output info:]

This compute calculates a per-particle vector, which can be accessed
by any command that uses per-particle values from a compute as input.
See "How-to discussions, section 6.15"_Section_howto.html#howto_15 for
an overview of LAMMPS output options.

The per-particle values will be given in "units"_units.html of time.

[Restrictions:]

This compute is part of the USER-SMD package.  It is only enabled if
LAMMPS was built with that package.  See the "Making
LAMMPS"_Section_start.html#start_3 section for more info.

This compute can only be used for particles interacting with the
Total-Lagrangian SPH pair style.

[Related commands:]

"smd/adjust/dt"_fix_smd_adjust_dt.html

[Default:] none
